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Wired indoor siren 

	· Adjustable volume of alarms and notifications

· Delay and security mode changing indication

· Two colours сasing

· Energy consumption up to 50 µA
	· Remote control and setup

· Adjustable alarm duration

· Door opening notifications

· External LED connection

· Fibra line connection up to 2,000 m



	HomeSiren Fibra — is the device of the new Fibra wired product line. Such devices can only be purchased, installed and administered by accredited Ajax partners.


[bookmark: _7940i3wp7vc6]Communication protocol Fibra 

The new wired line of Fibra devices has inherited all the advantages of the Jeweller wireless line. Data transmission that is encrypted and protected from sabotage, unprecedented range and energy efficiency, remote control and maintenance, the fastest possible installation. 

Fibra technology allows building complex protection regardless of facility size, steel or concrete obstructions. Security is enhanced by informative notifications, photo verification of alarms, real-time system control in the app, and automation scenarios.
[bookmark: _qkd34gte35cd]Adjustable volume of alarms and notifications

When alarmed, the siren sounds for 3 to 180 seconds, producing a sound volume of 85 to 113 dB. In the Ajax apps, you can set the duration and volume of the alarm, as well as determine which detectors will activate the siren.
[bookmark: _59y0egz8oypj]Chime

Chime is a sound signal that notifies about the triggering of the opening detectors when the system is disarmed. The feature is used, for example, in stores, to notify employees that someone has entered the building.
[bookmark: _35jbfyxgy3gb]Connecting an external LED

An external LED can be connected to HomeSiren Fibra. It works in parallel with the built-in LED of the device and fully repitess its signals.
[bookmark: _c46qz77t3zng]Technical specifications

	General settings

	Classification
	Light and sound siren

	Colour
	White
Black

	Installation method
	Indoors

	Type of detector
	Wired

	Limitations

	Compatibility
	Hub Hybrid (2G)
Hub Hybrid (4G)

	Communication

	Fibra protocol
	Transmission of events and alarms

Alarm delivery time: 0.15 s

	Recommended cable type for detector connection
	Signal cable (4×0.22, copper)
Twisted pair U/UTP cat.5 (4×2×0.51)

	Connection wire length
	Up to 2000 m

	Polling interval
	12 to 300 seconds

	Siren parameters

	Sound notification volume
	81–105 dB at 1 m distance (sets by admin in the app)

	Siren sound alert frequency
	3.4 ± 0.5 kHz

	Anti-sabotage protection

	Tampering alarm
	Yes

	Protection against forgery
	Yes

	Power supply

	Siren power supply
	24 V⎓, up to 3 A

	Current consumption
	TBC

	Enclosure

	Protection class
	IP50

	Operating temperature range
	From −10°C to +40°C

	Operating humidity
	Up to 75%

	Dimensions
	TBC

	Weight
	TBC

	Service life
	10 years



